<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.40.5-Bratislava">
  <identifier>Sant Cugat del Vallès</identifier>
  <parentidentifier>Topografia</parentidentifier>
  <language>Cat</language>
  <type>dataset</type>
  <title>Terme municipal</title>
  <abstract>Sant Cugat limita amb 8 termes municipals i s’han fet 7 delimitacions. Només falta Cerdanyola, aquest tram té més de 100 anys (és de 1917). La darrera delimitació que es va fer va ser Barcelona, al maig de 2022. Aquesta és la darrera vegada que hem modificat l’arxiu del límit (DOGC Núm. 8772 - 14.10.2022) </abstract>
  <contact>
    <name></name>
    <organization></organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email></email>
    <role></role>
  </contact>
  <links/>
  <dates/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["ETRS89 / UTM zone 31N",BASEGEOGCRS["ETRS89",ENSEMBLE["European Terrestrial Reference System 1989 ensemble",MEMBER["European Terrestrial Reference Frame 1989"],MEMBER["European Terrestrial Reference Frame 1990"],MEMBER["European Terrestrial Reference Frame 1991"],MEMBER["European Terrestrial Reference Frame 1992"],MEMBER["European Terrestrial Reference Frame 1993"],MEMBER["European Terrestrial Reference Frame 1994"],MEMBER["European Terrestrial Reference Frame 1996"],MEMBER["European Terrestrial Reference Frame 1997"],MEMBER["European Terrestrial Reference Frame 2000"],MEMBER["European Terrestrial Reference Frame 2005"],MEMBER["European Terrestrial Reference Frame 2014"],MEMBER["European Terrestrial Reference Frame 2020"],ELLIPSOID["GRS 1980",6378137,298.257222101,LENGTHUNIT["metre",1]],ENSEMBLEACCURACY[0.1]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4258]],CONVERSION["UTM zone 31N",METHOD["Transverse Mercator",ID["EPSG",9807]],PARAMETER["Latitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",3,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["Scale factor at natural origin",0.9996,SCALEUNIT["unity",1],ID["EPSG",8805]],PARAMETER["False easting",500000,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",0,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["(E)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["(N)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Engineering survey, topographic mapping."],AREA["Europe between 0°E and 6°E: Andorra; Denmark - offshore; Germany - offshore; Jan Mayen - offshore; Norway including Svalbard - onshore and offshore; Spain - mainland and Balearic islands - onshore and offshore."],BBOX[37,0,82.45,6.01]],USAGE[SCOPE["Pan-European conformal mapping at scales larger than 1:500,000."],AREA["Europe between 0°E and 6°E and approximately 37°N to 82°27'N."],BBOX[37,0,82.45,6.01]],ID["EPSG",25831]]</wkt>
      <proj4>+proj=utm +zone=31 +ellps=GRS80 +towgs84=0,0,0,0,0,0,0 +units=m +no_defs</proj4>
      <srsid>2104</srsid>
      <srid>25831</srid>
      <authid>EPSG:25831</authid>
      <description>ETRS89 / UTM zone 31N</description>
      <projectionacronym>utm</projectionacronym>
      <ellipsoidacronym>EPSG:7019</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial maxx="431557.00729999999748543" maxz="0" maxy="4597158.24330000020563602" dimensions="2" crs="EPSG:25831" minz="0" miny="4584938.75339999981224537" minx="412226.41279999999096617"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
